(kicad_pcb (version 20211014) (generator pcbnew)
  (general
    (thickness 1.6)
  )
  (paper "A4")
  (layers
    (0 "F.Cu" signal)
    (31 "B.Cu" signal)
    (32 "B.Adhes" user "B.Adhesive")
    (33 "F.Adhes" user "F.Adhesive")
    (34 "B.Paste" user)
    (35 "F.Paste" user)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (40 "Dwgs.User" user "User.Drawings")
    (41 "Cmts.User" user "User.Comments")
    (42 "Eco1.User" user "User.Eco1")
    (43 "Eco2.User" user "User.Eco2")
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
    (48 "B.Fab" user)
    (49 "F.Fab" user)
  )
  (setup
    (pad_to_mask_clearance 0)
    (pcbplotparams
      (layerselection 0x00010fc_ffffffff)
      (disableapertmacros false)
      (usegerberextensions true)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (svguseinch false)
      (svgprecision 6)
      (excludeedgelayer true)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (dxfpolygonmode true)
      (dxfimperialunits true)
      (dxfusepcbnewfont true)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue false)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk true)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "chargeur_piles_gerber")
    )
  )
  (net 0 "")
  (net 1 "Net-(A1-Pad17)")
  (net 2 "Net-(A1-Pad18)")
  (net 3 "Net-(A1-Pad20)")
  (net 4 "Net-(A1-Pad5)")
  (net 5 "Net-(A1-Pad22)")
  (net 6 "Net-(A1-Pad24)")
  (net 7 "Net-(A1-Pad9)")
  (net 8 "Net-(A1-Pad25)")
  (net 9 "GND")
  (net 10 "Net-(Q1-Pad1)")
  (net 11 "Net-(K1-Pad1)")
  (net 12 "Net-(Q1-Pad3)")
  (net 13 "Net-(D2-Pad2)")
  (net 14 "Net-(D3-Pad2)")
  (net 15 "Net-(A1-Pad7)")
  (net 16 "Net-(A1-Pad30)")
  (net 17 "Net-(A1-Pad27)")
  (footprint "Diode_THT:D_DO-41_SOD81_P10.16mm_Horizontal" (layer "F.Cu")
    (tedit 5AE50CD5)
    (at 146.685 109.728 90)
    (descr "Diode, DO-41_SOD81 series, Axial, Horizontal, pin pitch=10.16mm, , length*diameter=5.2*2.7mm^2, , http://www.diodes.com/_files/packages/DO-41%20(Plastic).pdf")
    (tags "Diode DO-41_SOD81 series Axial Horizontal pin pitch 10.16mm  length 5.2mm diameter 2.7mm")
    (attr through_hole)
    (fp_text reference "D1" (at 4.445 -2.667 90) (layer "F.SilkS"))
    (fp_text value "1N4001" (at 5.08 2.47 90) (layer "B.Fab"))
    (fp_text user "K" (at 0 -2.1 90) (layer "F.SilkS") hide)
    (fp_text user "${REFERENCE}" (at 4.445 -2.667 90) (layer "F.Fab") hide)
    (fp_text user "K" (at 0 -2.1 90) (layer "F.Fab") hide)
    (pad "1" thru_hole rect locked (at 0 0 90) (size 2.2 2.2) (drill 1.1) (layers *.Cu *.Mask)
      (net 8 "Net-(A1-Pad25)"))
    (pad "2" thru_hole oval locked (at 10.16 0 90) (size 2.2 2.2) (drill 1.1) (layers *.Cu *.Mask)
      (net 9 "GND"))
    (model "${KISYS3DMOD}/Diode_THT.3dshapes/D_DO-41_SOD81_P10.16mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Relay_THT:Relay_SPDT_SANYOU_SRD_Series_Form_C" (layer "F.Cu")
    (tedit 58FA3148)
    (at 151.765 103.632)
    (descr "relay Sanyou SRD series Form C http://www.sanyourelay.ca/public/products/pdf/SRD.pdf")
    (tags "relay Sanyu SRD form C")
    (attr through_hole)
    (fp_text reference "K1" (at 3.937 9.398) (layer "F.SilkS"))
    (fp_text value "SRD-5VDC" (at 8 -9.6) (layer "B.Fab"))
    (fp_text user "1" (at 0 -2.3) (layer "B.Fab") hide)
    (fp_text user "${REFERENCE}" (at 3.937 9.398) (layer "F.Fab"))
    (pad "1" thru_hole circle locked (at 0 0 90) (size 3 3) (drill 1.3) (layers *.Cu *.Mask)
      (net 11 "Net-(K1-Pad1)"))
    (pad "2" thru_hole circle locked (at 1.95 6.05 90) (size 2.5 2.5) (drill 1) (layers *.Cu *.Mask)
      (net 8 "Net-(A1-Pad25)"))
    (pad "3" thru_hole circle locked (at 14.15 6.05 90) (size 3 3) (drill 1.3) (layers *.Cu *.Mask)
      (net 4 "Net-(A1-Pad5)"))
    (pad "4" thru_hole circle locked (at 14.2 -6 90) (size 3 3) (drill 1.3) (layers *.Cu *.Mask))
    (pad "5" thru_hole circle locked (at 1.95 -5.95 90) (size 2.5 2.5) (drill 1) (layers *.Cu *.Mask)
      (net 9 "GND"))
    (model "${KISYS3DMOD}/Relay_THT.3dshapes/Relay_SPDT_SANYOU_SRD_Series_Form_C.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "kicad_chargeur_piles:Display_TM1637" (layer "F.Cu")
    (tedit 6254367B)
    (at 183.388 73.279 90)
    (descr "Through hole straight pin header, 1x04, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x04 2.54mm single row")
    (attr through_hole)
    (fp_text reference "U1" (at 0 11.43 90) (layer "F.SilkS"))
    (fp_text value "Display_TM1637" (at -24.13 5.08 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 11.43 270) (layer "F.Fab"))
    (pad "1" thru_hole rect locked (at 0 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 9 "GND"))
    (pad "2" thru_hole oval locked (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 "Net-(A1-Pad5)"))
    (pad "3" thru_hole oval locked (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 "Net-(A1-Pad17)"))
    (pad "4" thru_hole oval locked (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 "Net-(A1-Pad18)"))
    (model "${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x04_P2.54mm_Vertical.wrl"
      (offset (xyz -0.5 -0.5 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model "C:/Users/patri/Documents/Site electrotechnique/themes/chargeur_piles/kicad_chargeur_piles.pretty/display_4_7segment.step"
      (offset (xyz -40 -16.3 9))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "LED_THT:LED_D3.0mm" (layer "F.Cu")
    (tedit 587A3A7B)
    (at 172.085 87.249 90)
    (descr "LED, diameter 3.0mm, 2 pins")
    (tags "LED diameter 3.0mm 2 pins")
    (attr through_hole)
    (fp_text reference "D3" (at 4.318 0 180) (layer "F.SilkS"))
    (fp_text value "LED Rouge" (at -5.715 0 90) (layer "B.Fab"))
    (pad "1" thru_hole rect locked (at 0 0 90) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 9 "GND"))
    (pad "2" thru_hole circle locked (at 2.54 0 90) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 14 "Net-(D3-Pad2)"))
    (model "${KISYS3DMOD}/LED_THT.3dshapes/LED_D3.0mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "LED_THT:LED_D3.0mm" (layer "F.Cu")
    (tedit 587A3A7B)
    (at 167.259 87.249 90)
    (descr "LED, diameter 3.0mm, 2 pins")
    (tags "LED diameter 3.0mm 2 pins")
    (attr through_hole)
    (fp_text reference "D2" (at 4.318 -0.127 180) (layer "F.SilkS"))
    (fp_text value "LED verte" (at -4.445 0 90) (layer "B.Fab"))
    (pad "1" thru_hole rect locked (at 0 0 90) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 9 "GND"))
    (pad "2" thru_hole circle locked (at 2.54 0 90) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 13 "Net-(D2-Pad2)"))
    (model "${KISYS3DMOD}/LED_THT.3dshapes/LED_D3.0mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal" (layer "F.Cu")
    (tedit 5AE5139B)
    (at 172.212 73.152 -90)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (attr through_hole)
    (fp_text reference "R3" (at -2.794 0.889 90) (layer "F.SilkS"))
    (fp_text value "R_Small" (at 3.81 2.37 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at -2.794 0.889 90) (layer "F.Fab"))
    (pad "1" thru_hole circle locked (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 5 "Net-(A1-Pad22)"))
    (pad "2" thru_hole oval locked (at 7.62 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 14 "Net-(D3-Pad2)"))
    (model "${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal" (layer "F.Cu")
    (tedit 5AE5139B)
    (at 167.132 73.152 -90)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (attr through_hole)
    (fp_text reference "R2" (at -2.794 0.889 90) (layer "F.SilkS"))
    (fp_text value "R_Small" (at 3.81 2.37 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at -2.794 0.889 90) (layer "F.Fab"))
    (pad "1" thru_hole circle locked (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 6 "Net-(A1-Pad24)"))
    (pad "2" thru_hole oval locked (at 7.62 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 13 "Net-(D2-Pad2)"))
    (model "${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "TerminalBlock_Phoenix:TerminalBlock_Phoenix_MKDS-1,5-2_1x02_P5.00mm_Horizontal" (layer "F.Cu")
    (tedit 5B294EE5)
    (at 131.699 115.697)
    (descr "Terminal Block Phoenix MKDS-1,5-2, 2 pins, pitch 5mm, size 10x9.8mm^2, drill diamater 1.3mm, pad diameter 2.6mm, see http://www.farnell.com/datasheets/100425.pdf, script-generated using https://github.com/pointhi/kicad-footprint-generator/scripts/TerminalBlock_Phoenix")
    (tags "THT Terminal Block Phoenix MKDS-1,5-2 pitch 5mm size 10x9.8mm^2 drill 1.3mm pad 2.6mm")
    (attr through_hole)
    (fp_text reference "J1" (at 9.144 -0.127 180) (layer "F.SilkS"))
    (fp_text value "Conn_01x02" (at 2.159 3.302) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 9.144 -0.127 180) (layer "F.Fab"))
    (pad "1" thru_hole rect locked (at 0 0) (size 2.6 2.6) (drill 1.3) (layers *.Cu *.Mask)
      (net 7 "Net-(A1-Pad9)"))
    (pad "2" thru_hole circle locked (at 5 0) (size 2.6 2.6) (drill 1.3) (layers *.Cu *.Mask)
      (net 9 "GND"))
    (model "${KISYS3DMOD}/TerminalBlock_Phoenix.3dshapes/TerminalBlock_Phoenix_MKDS-1,5-2_1x02_P5.00mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_TO_SOT_THT:TO-220-3_Horizontal_TabDown" (layer "F.Cu")
    (tedit 5AC8BA0D)
    (at 137.668 88.646)
    (descr "TO-220-3, Horizontal, RM 2.54mm, see https://www.vishay.com/docs/66542/to-220-1.pdf")
    (tags "TO-220-3 Horizontal RM 2.54mm")
    (attr through_hole)
    (fp_text reference "Q1" (at -3.81 -12.7 -90) (layer "F.SilkS"))
    (fp_text value "Q_PMOS_GDS" (at 2.54 2) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at -3.81 -12.7 270) (layer "F.Fab"))
    (pad "" np_thru_hole oval locked (at 2.54 -16.66) (size 3.5 3.5) (drill 3.5) (layers *.Cu *.Mask))
    (pad "1" thru_hole rect locked (at 0 0) (size 1.905 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 10 "Net-(Q1-Pad1)"))
    (pad "2" thru_hole oval locked (at 2.54 0) (size 1.905 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 7 "Net-(A1-Pad9)"))
    (pad "3" thru_hole oval locked (at 5.08 0) (size 1.905 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 12 "Net-(Q1-Pad3)"))
    (model "${KISYS3DMOD}/Package_TO_SOT_THT.3dshapes/TO-220-3_Horizontal_TabDown.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal" (layer "F.Cu")
    (tedit 5AE5139B)
    (at 132.08 81.153 -90)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (attr through_hole)
    (fp_text reference "R6" (at 3.175 2.54 90) (layer "F.SilkS"))
    (fp_text value "R_Small" (at 3.81 2.37 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 3.175 2.54 90) (layer "F.Fab"))
    (pad "1" thru_hole circle locked (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 "Net-(A1-Pad20)"))
    (pad "2" thru_hole oval locked (at 7.62 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 10 "Net-(Q1-Pad1)"))
    (model "${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal" (layer "F.Cu")
    (tedit 5AE5139B)
    (at 140.335 92.964)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (attr through_hole)
    (fp_text reference "R1" (at 4.191 2.794) (layer "F.SilkS"))
    (fp_text value "R_Small" (at 3.81 2.37) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 4.191 2.794) (layer "F.Fab"))
    (pad "1" thru_hole circle locked (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 "Net-(A1-Pad9)"))
    (pad "2" thru_hole oval locked (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 9 "GND"))
    (model "${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal" (layer "F.Cu")
    (tedit 5AE5139B)
    (at 139.573 106.68 90)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (attr through_hole)
    (fp_text reference "R4" (at 4.572 -2.286 90) (layer "F.SilkS"))
    (fp_text value "R_Small" (at 3.81 2.37 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 4.572 -2.286 90) (layer "F.Fab"))
    (pad "1" thru_hole circle locked (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 11 "Net-(K1-Pad1)"))
    (pad "2" thru_hole oval locked (at 7.62 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 12 "Net-(Q1-Pad3)"))
    (model "${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal" (layer "F.Cu")
    (tedit 5AE5139B)
    (at 133.985 98.933 -90)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (attr through_hole)
    (fp_text reference "R5" (at 3.302 2.413 90) (layer "F.SilkS"))
    (fp_text value "R_Small" (at 3.81 2.37 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 3.302 2.413 90) (layer "F.Fab"))
    (pad "1" thru_hole circle locked (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 10 "Net-(Q1-Pad1)"))
    (pad "2" thru_hole oval locked (at 7.62 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 12 "Net-(Q1-Pad3)"))
    (model "${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_THT:C_Rect_L7.0mm_W2.0mm_P5.00mm" (layer "F.Cu")
    (tedit 5AE50EF0)
    (at 151.384 85.598 -90)
    (descr "C, Rect series, Radial, pin pitch=5.00mm, , length*width=7*2mm^2, Capacitor")
    (tags "C Rect series Radial pin pitch 5.00mm  length 7mm width 2mm Capacitor")
    (attr through_hole)
    (fp_text reference "C1" (at 2.032 2.286 90) (layer "F.SilkS"))
    (fp_text value "C" (at 2.5 2.25 90) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 2.032 2.286 90) (layer "F.Fab"))
    (pad "1" thru_hole circle locked (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 "Net-(A1-Pad9)"))
    (pad "2" thru_hole circle locked (at 5 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 9 "GND"))
    (model "${KISYS3DMOD}/Capacitor_THT.3dshapes/C_Rect_L7.0mm_W2.0mm_P5.00mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal" (layer "F.Cu")
    (tedit 5AE5139B)
    (at 164.465 92.456 180)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (attr through_hole)
    (fp_text reference "R7" (at 4.064 2.921) (layer "F.SilkS"))
    (fp_text value "R_Small" (at 3.81 2.37) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 4.064 2.921) (layer "F.Fab"))
    (pad "1" thru_hole circle locked (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 "Net-(A1-Pad5)"))
    (pad "2" thru_hole oval locked (at 7.62 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 16 "Net-(A1-Pad30)"))
    (model "${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_THT:CP_Radial_Tantal_D6.0mm_P2.50mm" (layer "F.Cu")
    (tedit 5AE50EF0)
    (at 156.845 83.947)
    (descr "CP, Radial_Tantal series, Radial, pin pitch=2.50mm, , diameter=6.0mm, Tantal Electrolytic Capacitor, http://cdn-reichelt.de/documents/datenblatt/B300/TANTAL-TB-Serie%23.pdf")
    (tags "CP Radial_Tantal series Radial pin pitch 2.50mm  diameter 6.0mm Tantal Electrolytic Capacitor")
    (attr through_hole)
    (fp_text reference "C2" (at -2.667 -2.54) (layer "F.SilkS"))
    (fp_text value "CP" (at 5.207 -1.778) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at -2.667 -2.54) (layer "F.Fab"))
    (pad "1" thru_hole rect locked (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 16 "Net-(A1-Pad30)"))
    (pad "2" thru_hole circle locked (at 2.5 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 15 "Net-(A1-Pad7)"))
    (model "${KISYS3DMOD}/Capacitor_THT.3dshapes/CP_Radial_Tantal_D6.0mm_P2.50mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_TO_SOT_THT:TO-92_Inline" (layer "F.Cu")
    (tedit 5A1DD157)
    (at 156.845 77.216)
    (descr "TO-92 leads in-line, narrow, oval pads, drill 0.75mm (see NXP sot054_po.pdf)")
    (tags "to-92 sc-43 sc-43a sot54 PA33 transistor")
    (attr through_hole)
    (fp_text reference "U2" (at -2.921 -0.381) (layer "F.SilkS"))
    (fp_text value "TL431LP" (at 1.27 3.594999) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at -2.921 -0.381) (layer "F.Fab"))
    (pad "1" thru_hole rect locked (at 0 0) (size 1.05 1.5) (drill 0.75) (layers *.Cu *.Mask)
      (net 16 "Net-(A1-Pad30)"))
    (pad "2" thru_hole oval locked (at 1.27 0) (size 1.05 1.5) (drill 0.75) (layers *.Cu *.Mask)
      (net 15 "Net-(A1-Pad7)"))
    (pad "3" thru_hole oval locked (at 2.54 0) (size 1.05 1.5) (drill 0.75) (layers *.Cu *.Mask)
      (net 16 "Net-(A1-Pad30)"))
    (model "${KISYS3DMOD}/Package_TO_SOT_THT.3dshapes/TO-92_Inline.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinHeader_1.00mm:PinHeader_1x02_P1.00mm_Vertical" (layer "F.Cu")
    (tedit 59FED738)
    (at 158.369 71.882 -90)
    (descr "Through hole straight pin header, 1x02, 1.00mm pitch, single row")
    (tags "Through hole pin header THT 1x02 1.00mm single row")
    (attr through_hole)
    (fp_text reference "TP1" (at -0.381 -2.794 180) (layer "F.SilkS"))
    (fp_text value "TestPoint_2Pole" (at 0 2.56 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at -0.381 -2.794) (layer "F.Fab"))
    (pad "1" thru_hole rect locked (at 0 0 270) (size 0.85 0.85) (drill 0.5) (layers *.Cu *.Mask)
      (net 17 "Net-(A1-Pad27)"))
    (pad "2" thru_hole oval locked (at 0 1 270) (size 0.85 0.85) (drill 0.5) (layers *.Cu *.Mask)
      (net 9 "GND"))
    (model "${KISYS3DMOD}/Connector_PinHeader_1.00mm.3dshapes/PinHeader_1x02_P1.00mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "kicad_chargeur_piles:Arduino_UNO_R3" (layer "B.Cu")
    (tedit 6252EFBB)
    (at 156.083 116.205)
    (descr "Arduino UNO R3, http://www.mouser.com/pdfdocs/Gravitech_Arduino_Nano3_0.pdf")
    (tags "Arduino UNO R3")
    (attr through_hole)
    (fp_text reference "A1" (at -2.794 0 180) (layer "F.SilkS"))
    (fp_text value "Arduino_UNO_R3" (at -5.207 2.794) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at -19.05 -48.26 -180) (layer "B.Fab"))
    (pad "1" thru_hole rect locked (at 0 0 270) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask))
    (pad "2" thru_hole oval locked (at 2.54 0 270) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask))
    (pad "3" thru_hole oval locked (at 5.08 0 270) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask))
    (pad "4" thru_hole oval locked (at 7.62 0 270) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask))
    (pad "5" thru_hole oval locked (at 10.16 0 270) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 4 "Net-(A1-Pad5)"))
    (pad "6" thru_hole oval locked (at 12.7 0 270) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask))
    (pad "7" thru_hole oval locked (at 15.24 0 270) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 15 "Net-(A1-Pad7)"))
    (pad "8" thru_hole oval locked (at 17.78 0 270) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask))
    (pad "9" thru_hole oval locked (at 22.86 0 270) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 7 "Net-(A1-Pad9)"))
    (pad "10" thru_hole oval locked (at 25.4 0 270) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask))
    (pad "11" thru_hole oval locked (at 27.94 0 270) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask))
    (pad "12" thru_hole oval locked (at 30.48 0 270) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask))
    (pad "13" thru_hole oval locked (at 33.02 0 270) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask))
    (pad "14" thru_hole oval locked (at 35.56 0 270) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask))
    (pad "15" thru_hole oval locked (at 35.56 -48.26 270) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask))
    (pad "16" thru_hole oval locked (at 33.02 -48.26 270) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask))
    (pad "17" thru_hole oval locked (at 30.48 -48.26 270) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 1 "Net-(A1-Pad17)"))
    (pad "18" thru_hole oval locked (at 27.94 -48.26 270) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 2 "Net-(A1-Pad18)"))
    (pad "19" thru_hole oval locked (at 25.4 -48.26 270) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask))
    (pad "20" thru_hole oval locked (at 22.86 -48.26 270) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 3 "Net-(A1-Pad20)"))
    (pad "21" thru_hole oval locked (at 20.32 -48.26 270) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask))
    (pad "22" thru_hole oval locked (at 17.78 -48.26 270) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 5 "Net-(A1-Pad22)"))
    (pad "23" thru_hole oval locked (at 13.72 -48.26 270) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask))
    (pad "24" thru_hole oval locked (at 11.18 -48.26 270) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 6 "Net-(A1-Pad24)"))
    (pad "25" thru_hole oval locked (at 8.64 -48.26 270) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 8 "Net-(A1-Pad25)"))
    (pad "26" thru_hole oval locked (at 6.1 -48.26 270) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask))
    (pad "27" thru_hole oval locked (at 3.56 -48.26 270) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 17 "Net-(A1-Pad27)"))
    (pad "28" thru_hole oval locked (at 1.02 -48.26 270) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask))
    (pad "29" thru_hole oval locked (at -1.52 -48.26 270) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 9 "GND"))
    (pad "30" thru_hole oval locked (at -4.06 -48.26 270) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 16 "Net-(A1-Pad30)"))
    (pad "31" thru_hole oval locked (at -6.6 -48.26 270) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask))
    (pad "32" thru_hole oval locked (at -9.14 -48.26 270) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask))
    (model "${KISYS3DMOD}/Module.3dshapes/Arduino_UNO_R3.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_rect (start 126.4 62.6) (end 200.8 121.6) (layer "Edge.Cuts") (width 0.1) (fill none))
  (gr_text "JLCJLCJLCJLC" (at 194.4 120) (layer "B.SilkS"))
  (gr_text "+ PILE -" (at 133.985 108.966) (layer "F.Fab"))
  (gr_text "Charge" (at 166.878 92.202 90) (layer "F.Fab"))
  (gr_text "Défaut" (at 171.958 92.202 90) (layer "F.Fab"))
  (zone (net 9) (net_name "GND") (layer "F.Cu") (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 200.406 121.158)
        (xy 126.873 121.158)
        (xy 126.873 63.119)
        (xy 200.406 63.119)
      )
    )
  )
)
