(kicad_sch (version 20211123) (generator eeschema)
  (paper "A4")
  (lib_symbols
    (symbol "Connector:TestPoint_2Pole" (pin_names (offset 0.762) hide) (in_bom yes) (on_board yes)
      (property "Reference" "TP" (id 0) (at 0 1.524 0))
      (property "Value" "TestPoint_2Pole" (id 1) (at 0 -1.778 0))
      (property "Footprint" "" (id 2) (at 0 0 0))
      (property "Datasheet" "~" (id 3) (at 0 0 0))
      (property "ki_keywords" "point tp" (id 4) (at 0 0 0))
      (property "ki_description" "2-polar test point" (id 5) (at 0 0 0))
      (property "ki_fp_filters" "Pin* Test*" (id 6) (at 0 0 0))
      (symbol "TestPoint_2Pole_0_1"
        (circle (center -1.778 0) (radius 0.762)
          (fill (type none))
        )
        (circle (center 1.778 0) (radius 0.762)
          (fill (type none))
        )
        (pin passive line (at -5.08 0 0) (length 2.54)
          (name "1")
          (number "1")
        )
        (pin passive line (at 5.08 0 180) (length 2.54)
          (name "2")
          (number "2")
        )
      )
    )
    (symbol "Connector_Generic:Conn_01x02" (pin_names (offset 1.016) hide) (in_bom yes) (on_board yes)
      (property "Reference" "J" (id 0) (at 0 2.54 0))
      (property "Value" "Conn_01x02" (id 1) (at 0 -5.08 0))
      (property "Footprint" "" (id 2) (at 0 0 0))
      (property "Datasheet" "~" (id 3) (at 0 0 0))
      (property "ki_keywords" "connector" (id 4) (at 0 0 0))
      (property "ki_description" "Generic connector, single row, 01x02, script generated (kicad-library-utils/schlib/autogen/connector/)" (id 5) (at 0 0 0))
      (property "ki_fp_filters" "Connector*:*_1x??_*" (id 6) (at 0 0 0))
      (symbol "Conn_01x02_1_1"
        (rectangle (start -1.27 -2.413) (end 0 -2.667)
          (fill (type none))
        )
        (rectangle (start -1.27 0.127) (end 0 -0.127)
          (fill (type none))
        )
        (rectangle (start -1.27 1.27) (end 1.27 -3.81)
          (fill (type background))
        )
        (pin passive line (at -5.08 0 0) (length 3.81)
          (name "Pin_1")
          (number "1")
        )
        (pin passive line (at -5.08 -2.54 0) (length 3.81)
          (name "Pin_2")
          (number "2")
        )
      )
    )
    (symbol "Device:C" (pin_numbers hide) (pin_names (offset 0.254)) (in_bom yes) (on_board yes)
      (property "Reference" "C" (id 0) (at 0.635 2.54 0))
      (property "Value" "C" (id 1) (at 0.635 -2.54 0))
      (property "Footprint" "" (id 2) (at 0.9652 -3.81 0))
      (property "Datasheet" "~" (id 3) (at 0 0 0))
      (property "ki_keywords" "cap capacitor" (id 4) (at 0 0 0))
      (property "ki_description" "Unpolarized capacitor" (id 5) (at 0 0 0))
      (property "ki_fp_filters" "C_*" (id 6) (at 0 0 0))
      (symbol "C_0_1"
        (polyline
          (pts
            (xy -2.032 -0.762)
            (xy 2.032 -0.762)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -2.032 0.762)
            (xy 2.032 0.762)
          )
          (fill (type none))
        )
      )
      (symbol "C_1_1"
        (pin passive line (at 0 3.81 270) (length 2.794)
          (name "~")
          (number "1")
        )
        (pin passive line (at 0 -3.81 90) (length 2.794)
          (name "~")
          (number "2")
        )
      )
    )
    (symbol "Device:C_Polarized" (pin_numbers hide) (pin_names (offset 0.254)) (in_bom yes) (on_board yes)
      (property "Reference" "C" (id 0) (at 0.635 2.54 0))
      (property "Value" "C_Polarized" (id 1) (at 0.635 -2.54 0))
      (property "Footprint" "" (id 2) (at 0.9652 -3.81 0))
      (property "Datasheet" "~" (id 3) (at 0 0 0))
      (property "ki_keywords" "cap capacitor" (id 4) (at 0 0 0))
      (property "ki_description" "Polarized capacitor" (id 5) (at 0 0 0))
      (property "ki_fp_filters" "CP_*" (id 6) (at 0 0 0))
      (symbol "C_Polarized_0_1"
        (rectangle (start -2.286 0.508) (end 2.286 1.016)
          (fill (type none))
        )
        (polyline
          (pts
            (xy -1.778 2.286)
            (xy -0.762 2.286)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -1.27 2.794)
            (xy -1.27 1.778)
          )
          (fill (type none))
        )
        (rectangle (start 2.286 -0.508) (end -2.286 -1.016)
          (fill (type outline))
        )
      )
      (symbol "C_Polarized_1_1"
        (pin passive line (at 0 3.81 270) (length 2.794)
          (name "~")
          (number "1")
        )
        (pin passive line (at 0 -3.81 90) (length 2.794)
          (name "~")
          (number "2")
        )
      )
    )
    (symbol "Device:LED" (pin_numbers hide) (pin_names (offset 1.016) hide) (in_bom yes) (on_board yes)
      (property "Reference" "D" (id 0) (at 0 2.54 0))
      (property "Value" "LED" (id 1) (at 0 -2.54 0))
      (property "Footprint" "" (id 2) (at 0 0 0))
      (property "Datasheet" "~" (id 3) (at 0 0 0))
      (property "ki_keywords" "LED diode" (id 4) (at 0 0 0))
      (property "ki_description" "Light emitting diode" (id 5) (at 0 0 0))
      (property "ki_fp_filters" "LED* LED_SMD:* LED_THT:*" (id 6) (at 0 0 0))
      (symbol "LED_0_1"
        (polyline
          (pts
            (xy -1.27 -1.27)
            (xy -1.27 1.27)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -1.27 0)
            (xy 1.27 0)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 1.27 -1.27)
            (xy 1.27 1.27)
            (xy -1.27 0)
            (xy 1.27 -1.27)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -3.048 -0.762)
            (xy -4.572 -2.286)
            (xy -3.81 -2.286)
            (xy -4.572 -2.286)
            (xy -4.572 -1.524)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -1.778 -0.762)
            (xy -3.302 -2.286)
            (xy -2.54 -2.286)
            (xy -3.302 -2.286)
            (xy -3.302 -1.524)
          )
          (fill (type none))
        )
      )
      (symbol "LED_1_1"
        (pin passive line (at -3.81 0 0) (length 2.54)
          (name "K")
          (number "1")
        )
        (pin passive line (at 3.81 0 180) (length 2.54)
          (name "A")
          (number "2")
        )
      )
    )
    (symbol "Device:Q_PMOS_GDS" (pin_names (offset 0) hide) (in_bom yes) (on_board yes)
      (property "Reference" "Q" (id 0) (at 5.08 1.27 0))
      (property "Value" "Q_PMOS_GDS" (id 1) (at 5.08 -1.27 0))
      (property "Footprint" "" (id 2) (at 5.08 2.54 0))
      (property "Datasheet" "~" (id 3) (at 0 0 0))
      (property "ki_keywords" "transistor PMOS P-MOS P-MOSFET" (id 4) (at 0 0 0))
      (property "ki_description" "P-MOSFET transistor, gate/drain/source" (id 5) (at 0 0 0))
      (symbol "Q_PMOS_GDS_0_1"
        (polyline
          (pts
            (xy 0.254 0)
            (xy -2.54 0)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 0.254 1.905)
            (xy 0.254 -1.905)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 0.762 -1.27)
            (xy 0.762 -2.286)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 0.762 0.508)
            (xy 0.762 -0.508)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 0.762 2.286)
            (xy 0.762 1.27)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 2.54 2.54)
            (xy 2.54 1.778)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 2.54 -2.54)
            (xy 2.54 0)
            (xy 0.762 0)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 0.762 1.778)
            (xy 3.302 1.778)
            (xy 3.302 -1.778)
            (xy 0.762 -1.778)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 2.286 0)
            (xy 1.27 0.381)
            (xy 1.27 -0.381)
            (xy 2.286 0)
          )
          (fill (type outline))
        )
        (polyline
          (pts
            (xy 2.794 -0.508)
            (xy 2.921 -0.381)
            (xy 3.683 -0.381)
            (xy 3.81 -0.254)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 3.302 -0.381)
            (xy 2.921 0.254)
            (xy 3.683 0.254)
            (xy 3.302 -0.381)
          )
          (fill (type none))
        )
        (circle (center 1.651 0) (radius 2.794)
          (fill (type none))
        )
        (circle (center 2.54 -1.778) (radius 0.254)
          (fill (type outline))
        )
        (circle (center 2.54 1.778) (radius 0.254)
          (fill (type outline))
        )
      )
      (symbol "Q_PMOS_GDS_1_1"
        (pin input line (at -5.08 0 0) (length 2.54)
          (name "G")
          (number "1")
        )
        (pin passive line (at 2.54 5.08 270) (length 2.54)
          (name "D")
          (number "2")
        )
        (pin passive line (at 2.54 -5.08 90) (length 2.54)
          (name "S")
          (number "3")
        )
      )
    )
    (symbol "Device:R_Small" (pin_numbers hide) (pin_names (offset 0.254) hide) (in_bom yes) (on_board yes)
      (property "Reference" "R" (id 0) (at 0.762 0.508 0))
      (property "Value" "R_Small" (id 1) (at 0.762 -1.016 0))
      (property "Footprint" "" (id 2) (at 0 0 0))
      (property "Datasheet" "~" (id 3) (at 0 0 0))
      (property "ki_keywords" "R resistor" (id 4) (at 0 0 0))
      (property "ki_description" "Resistor, small symbol" (id 5) (at 0 0 0))
      (property "ki_fp_filters" "R_*" (id 6) (at 0 0 0))
      (symbol "R_Small_0_1"
        (rectangle (start -0.762 1.778) (end 0.762 -1.778)
          (fill (type none))
        )
      )
      (symbol "R_Small_1_1"
        (pin passive line (at 0 2.54 270) (length 0.762)
          (name "~")
          (number "1")
        )
        (pin passive line (at 0 -2.54 90) (length 0.762)
          (name "~")
          (number "2")
        )
      )
    )
    (symbol "Diode:1N4004" (pin_numbers hide) (pin_names (offset 1.016) hide) (in_bom yes) (on_board yes)
      (property "Reference" "D" (id 0) (at 0 2.54 0))
      (property "Value" "1N4004" (id 1) (at 0 -2.54 0))
      (property "Footprint" "Diode_THT:D_DO-41_SOD81_P10.16mm_Horizontal" (id 2) (at 0 -4.445 0))
      (property "Datasheet" "http://www.vishay.com/docs/88503/1n4001.pdf" (id 3) (at 0 0 0))
      (property "ki_keywords" "diode" (id 4) (at 0 0 0))
      (property "ki_description" "400V 1A General Purpose Rectifier Diode, DO-41" (id 5) (at 0 0 0))
      (property "ki_fp_filters" "D*DO?41*" (id 6) (at 0 0 0))
      (symbol "1N4004_0_1"
        (polyline
          (pts
            (xy -1.27 1.27)
            (xy -1.27 -1.27)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 1.27 0)
            (xy -1.27 0)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 1.27 1.27)
            (xy 1.27 -1.27)
            (xy -1.27 0)
            (xy 1.27 1.27)
          )
          (fill (type none))
        )
      )
      (symbol "1N4004_1_1"
        (pin passive line (at -3.81 0 0) (length 2.54)
          (name "K")
          (number "1")
        )
        (pin passive line (at 3.81 0 180) (length 2.54)
          (name "A")
          (number "2")
        )
      )
    )
    (symbol "MCU_Module:Arduino_UNO_R3" (in_bom yes) (on_board yes)
      (property "Reference" "A" (id 0) (at -10.16 23.495 0))
      (property "Value" "Arduino_UNO_R3" (id 1) (at 5.08 -26.67 0))
      (property "Footprint" "Module:Arduino_UNO_R3" (id 2) (at 0 0 0))
      (property "Datasheet" "https://www.arduino.cc/en/Main/arduinoBoardUno" (id 3) (at 0 0 0))
      (property "ki_keywords" "Arduino UNO R3 Microcontroller Module Atmel AVR USB" (id 4) (at 0 0 0))
      (property "ki_description" "Arduino UNO Microcontroller Module, release 3" (id 5) (at 0 0 0))
      (property "ki_fp_filters" "Arduino*UNO*R3*" (id 6) (at 0 0 0))
      (symbol "Arduino_UNO_R3_0_1"
        (rectangle (start -10.16 22.86) (end 10.16 -25.4)
          (fill (type background))
        )
      )
      (symbol "Arduino_UNO_R3_1_1"
        (pin no_connect line (at -10.16 -20.32 0) (length 2.54) hide
          (name "NC")
          (number "1")
        )
        (pin bidirectional line (at 12.7 -2.54 180) (length 2.54)
          (name "A1")
          (number "10")
        )
        (pin bidirectional line (at 12.7 -5.08 180) (length 2.54)
          (name "A2")
          (number "11")
        )
        (pin bidirectional line (at 12.7 -7.62 180) (length 2.54)
          (name "A3")
          (number "12")
        )
        (pin bidirectional line (at 12.7 -10.16 180) (length 2.54)
          (name "SDA/A4")
          (number "13")
        )
        (pin bidirectional line (at 12.7 -12.7 180) (length 2.54)
          (name "SCL/A5")
          (number "14")
        )
        (pin bidirectional line (at -12.7 15.24 0) (length 2.54)
          (name "D0/RX")
          (number "15")
        )
        (pin bidirectional line (at -12.7 12.7 0) (length 2.54)
          (name "D1/TX")
          (number "16")
        )
        (pin bidirectional line (at -12.7 10.16 0) (length 2.54)
          (name "D2")
          (number "17")
        )
        (pin bidirectional line (at -12.7 7.62 0) (length 2.54)
          (name "D3")
          (number "18")
        )
        (pin bidirectional line (at -12.7 5.08 0) (length 2.54)
          (name "D4")
          (number "19")
        )
        (pin output line (at 12.7 10.16 180) (length 2.54)
          (name "IOREF")
          (number "2")
        )
        (pin bidirectional line (at -12.7 2.54 0) (length 2.54)
          (name "D5")
          (number "20")
        )
        (pin bidirectional line (at -12.7 0 0) (length 2.54)
          (name "D6")
          (number "21")
        )
        (pin bidirectional line (at -12.7 -2.54 0) (length 2.54)
          (name "D7")
          (number "22")
        )
        (pin bidirectional line (at -12.7 -5.08 0) (length 2.54)
          (name "D8")
          (number "23")
        )
        (pin bidirectional line (at -12.7 -7.62 0) (length 2.54)
          (name "D9")
          (number "24")
        )
        (pin bidirectional line (at -12.7 -10.16 0) (length 2.54)
          (name "D10")
          (number "25")
        )
        (pin bidirectional line (at -12.7 -12.7 0) (length 2.54)
          (name "D11")
          (number "26")
        )
        (pin bidirectional line (at -12.7 -15.24 0) (length 2.54)
          (name "D12")
          (number "27")
        )
        (pin bidirectional line (at -12.7 -17.78 0) (length 2.54)
          (name "D13")
          (number "28")
        )
        (pin power_in line (at -2.54 -27.94 90) (length 2.54)
          (name "GND")
          (number "29")
        )
        (pin input line (at 12.7 15.24 180) (length 2.54)
          (name "~{RESET}")
          (number "3")
        )
        (pin input line (at 12.7 5.08 180) (length 2.54)
          (name "AREF")
          (number "30")
        )
        (pin bidirectional line (at 12.7 -17.78 180) (length 2.54)
          (name "SDA/A4")
          (number "31")
        )
        (pin bidirectional line (at 12.7 -20.32 180) (length 2.54)
          (name "SCL/A5")
          (number "32")
        )
        (pin power_out line (at 2.54 25.4 270) (length 2.54)
          (name "3V3")
          (number "4")
        )
        (pin power_out line (at 5.08 25.4 270) (length 2.54)
          (name "+5V")
          (number "5")
        )
        (pin power_in line (at 0 -27.94 90) (length 2.54)
          (name "GND")
          (number "6")
        )
        (pin power_in line (at 2.54 -27.94 90) (length 2.54)
          (name "GND")
          (number "7")
        )
        (pin power_in line (at -2.54 25.4 270) (length 2.54)
          (name "VIN")
          (number "8")
        )
        (pin bidirectional line (at 12.7 0 180) (length 2.54)
          (name "A0")
          (number "9")
        )
      )
    )
    (symbol "Reference_Voltage:TL431LP" (pin_numbers hide) (pin_names hide) (in_bom yes) (on_board yes)
      (property "Reference" "U" (id 0) (at -2.54 2.54 0))
      (property "Value" "TL431LP" (id 1) (at 0 -2.54 0))
      (property "Footprint" "Package_TO_SOT_THT:TO-92_Inline" (id 2) (at 0 -3.81 0))
      (property "Datasheet" "http://www.ti.com/lit/ds/symlink/tl431.pdf" (id 3) (at 0 0 0))
      (property "ki_keywords" "diode device regulator shunt" (id 4) (at 0 0 0))
      (property "ki_description" "Shunt Regulator, TO-92" (id 5) (at 0 0 0))
      (property "ki_fp_filters" "TO*92*" (id 6) (at 0 0 0))
      (symbol "TL431LP_0_1"
        (polyline
          (pts
            (xy -1.27 0)
            (xy 0 0)
            (xy 1.27 0)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -0.762 0.762)
            (xy 0.762 0)
            (xy -0.762 -0.762)
          )
          (fill (type outline))
        )
        (polyline
          (pts
            (xy 0.508 -1.016)
            (xy 0.762 -0.762)
            (xy 0.762 0.762)
            (xy 0.762 0.762)
          )
          (fill (type none))
        )
      )
      (symbol "TL431LP_1_1"
        (pin passive line (at 0 2.54 270) (length 2.54)
          (name "REF")
          (number "1")
        )
        (pin passive line (at -2.54 0 0) (length 2.54)
          (name "A")
          (number "2")
        )
        (pin passive line (at 2.54 0 180) (length 2.54)
          (name "K")
          (number "3")
        )
      )
    )
    (symbol "Relay:SANYOU_SRD_Form_C" (in_bom yes) (on_board yes)
      (property "Reference" "K" (id 0) (at 11.43 3.81 0))
      (property "Value" "SANYOU_SRD_Form_C" (id 1) (at 11.43 1.27 0))
      (property "Footprint" "Relay_THT:Relay_SPDT_SANYOU_SRD_Series_Form_C" (id 2) (at 11.43 -1.27 0))
      (property "Datasheet" "http://www.sanyourelay.ca/public/products/pdf/SRD.pdf" (id 3) (at 0 0 0))
      (property "ki_keywords" "Single Pole Relay SPDT" (id 4) (at 0 0 0))
      (property "ki_description" "Sanyo SRD relay, Single Pole Miniature Power Relay," (id 5) (at 0 0 0))
      (property "ki_fp_filters" "Relay*SPDT*SANYOU*SRD*Series*Form*C*" (id 6) (at 0 0 0))
      (symbol "SANYOU_SRD_Form_C_0_0"
        (polyline
          (pts
            (xy 7.62 5.08)
            (xy 7.62 2.54)
            (xy 6.985 3.175)
            (xy 7.62 3.81)
          )
          (fill (type none))
        )
      )
      (symbol "SANYOU_SRD_Form_C_0_1"
        (rectangle (start -10.16 5.08) (end 10.16 -5.08)
          (fill (type background))
        )
        (rectangle (start -8.255 1.905) (end -1.905 -1.905)
          (fill (type none))
        )
        (polyline
          (pts
            (xy -7.62 -1.905)
            (xy -2.54 1.905)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -5.08 -5.08)
            (xy -5.08 -1.905)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -5.08 5.08)
            (xy -5.08 1.905)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -1.905 0)
            (xy -1.27 0)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -0.635 0)
            (xy 0 0)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 0.635 0)
            (xy 1.27 0)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 1.905 0)
            (xy 2.54 0)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 3.175 0)
            (xy 3.81 0)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 5.08 -2.54)
            (xy 3.175 3.81)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 5.08 -2.54)
            (xy 5.08 -5.08)
          )
          (fill (type none))
        )
      )
      (symbol "SANYOU_SRD_Form_C_1_1"
        (polyline
          (pts
            (xy 2.54 3.81)
            (xy 3.175 3.175)
            (xy 2.54 2.54)
            (xy 2.54 5.08)
          )
          (fill (type outline))
        )
        (pin passive line (at 5.08 -7.62 90) (length 2.54)
          (name "~")
          (number "1")
        )
        (pin passive line (at -5.08 -7.62 90) (length 2.54)
          (name "~")
          (number "2")
        )
        (pin passive line (at 7.62 7.62 270) (length 2.54)
          (name "~")
          (number "3")
        )
        (pin passive line (at 2.54 7.62 270) (length 2.54)
          (name "~")
          (number "4")
        )
        (pin passive line (at -5.08 7.62 270) (length 2.54)
          (name "~")
          (number "5")
        )
      )
    )
    (symbol "kicad_chargeur_piles_mosfet-rescue:Display_TM1637-display_tm1637-kicad_chargeur_piles-rescue" (in_bom yes) (on_board yes)
      (property "Reference" "U" (id 0) (at -24.13 13.97 0))
      (property "Value" "Display_TM1637-display_tm1637-kicad_chargeur_piles-rescue" (id 1) (at 17.78 13.97 0))
      (property "Footprint" "Display_4Digit_7Segment" (id 2) (at 0 -15.24 0))
      (property "Datasheet" "" (id 3) (at -10.922 0.762 0))
      (property "ki_fp_filters" "*CA56*12CGKWA*" (id 4) (at 0 0 0))
      (symbol "Display_TM1637-display_tm1637-kicad_chargeur_piles-rescue_0_0"
        (rectangle (start -25.4 12.7) (end 25.4 -12.7)
          (fill (type background))
        )
        (polyline
          (pts
            (xy -20.32 -3.81)
            (xy -19.05 0)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -19.05 -3.81)
            (xy -16.51 -3.81)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -18.796 1.27)
            (xy -17.526 5.08)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -17.78 0)
            (xy -15.24 0)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -16.256 5.08)
            (xy -13.716 5.08)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -15.24 -3.81)
            (xy -13.97 0)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -13.716 1.27)
            (xy -12.446 5.08)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -8.89 -3.81)
            (xy -7.62 0)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -7.62 -3.81)
            (xy -5.08 -3.81)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -7.366 1.27)
            (xy -6.096 5.08)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -6.35 0)
            (xy -3.81 0)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -4.826 5.08)
            (xy -2.286 5.08)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -3.81 -3.81)
            (xy -2.54 0)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -2.286 1.27)
            (xy -1.016 5.08)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 1.27 -3.81)
            (xy 2.54 0)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 2.54 -3.81)
            (xy 5.08 -3.81)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 2.794 1.27)
            (xy 4.064 5.08)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 3.81 0)
            (xy 6.35 0)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 5.334 5.08)
            (xy 7.874 5.08)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 6.35 -3.81)
            (xy 7.62 0)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 7.874 1.27)
            (xy 9.144 5.08)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 11.176 -3.81)
            (xy 12.446 0)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 12.446 -3.81)
            (xy 14.986 -3.81)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 12.7 1.27)
            (xy 13.97 5.08)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 13.716 0)
            (xy 16.256 0)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 15.24 5.08)
            (xy 17.78 5.08)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 16.256 -3.81)
            (xy 17.526 0)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 17.78 1.27)
            (xy 19.05 5.08)
          )
          (fill (type none))
        )
      )
      (symbol "Display_TM1637-display_tm1637-kicad_chargeur_piles-rescue_0_1"
        (circle (center 0 -1.27) (radius 0.3556)
          (fill (type outline))
        )
        (circle (center 0.254 2.54) (radius 0.3556)
          (fill (type outline))
        )
      )
      (symbol "Display_TM1637-display_tm1637-kicad_chargeur_piles-rescue_1_1"
        (pin passive line (at 27.94 -2.54 180) (length 2.54)
          (name "GND")
          (number "1")
        )
        (pin passive line (at 27.94 -5.08 180) (length 2.54)
          (name "VCC")
          (number "2")
        )
        (pin passive line (at 27.94 -7.62 180) (length 2.54)
          (name "DIO")
          (number "3")
        )
        (pin passive line (at 27.94 -10.16 180) (length 2.54)
          (name "CLK")
          (number "4")
        )
      )
    )
    (symbol "power:GND" (power) (pin_names (offset 0)) (in_bom yes) (on_board yes)
      (property "Reference" "#PWR" (id 0) (at 0 -6.35 0))
      (property "Value" "GND" (id 1) (at 0 -3.81 0))
      (property "Footprint" "" (id 2) (at 0 0 0))
      (property "Datasheet" "" (id 3) (at 0 0 0))
      (property "ki_keywords" "power-flag" (id 4) (at 0 0 0))
      (property "ki_description" "Power symbol creates a global label with name \"GND\" , ground" (id 5) (at 0 0 0))
      (symbol "GND_0_1"
        (polyline
          (pts
            (xy 0 0)
            (xy 0 -1.27)
            (xy 1.27 -1.27)
            (xy 0 -2.54)
            (xy -1.27 -1.27)
            (xy 0 -1.27)
          )
          (fill (type none))
        )
      )
      (symbol "GND_1_1"
        (pin power_in line (at 0 0 270) (length 0) hide
          (name "GND")
          (number "1")
        )
      )
    )
  )
  (junction (at 238.76 125.73) (diameter 0) (color 0 0 0 0))
  (junction (at 114.3 67.31) (diameter 0) (color 0 0 0 0))
  (junction (at 208.28 44.45) (diameter 0) (color 0 0 0 0))
  (junction (at 146.05 121.92) (diameter 0) (color 0 0 0 0))
  (junction (at 208.28 87.63) (diameter 0) (color 0 0 0 0))
  (junction (at 184.15 26.67) (diameter 0) (color 0 0 0 0))
  (junction (at 205.74 54.61) (diameter 0) (color 0 0 0 0))
  (junction (at 209.55 139.7) (diameter 0) (color 0 0 0 0))
  (junction (at 114.3 90.17) (diameter 0) (color 0 0 0 0))
  (junction (at 118.11 54.61) (diameter 0) (color 0 0 0 0))
  (junction (at 125.73 153.67) (diameter 0) (color 0 0 0 0))
  (junction (at 220.98 139.7) (diameter 0) (color 0 0 0 0))
  (junction (at 209.55 153.67) (diameter 0) (color 0 0 0 0))
  (junction (at 146.05 153.67) (diameter 0) (color 0 0 0 0))
  (junction (at 114.3 62.23) (diameter 0) (color 0 0 0 0))
  (junction (at 262.89 125.73) (diameter 0) (color 0 0 0 0))
  (junction (at 208.28 52.07) (diameter 0) (color 0 0 0 0))
  (junction (at 220.98 153.67) (diameter 0) (color 0 0 0 0))
  (junction (at 153.67 90.17) (diameter 0) (color 0 0 0 0))
  (junction (at 238.76 139.7) (diameter 0) (color 0 0 0 0))
  (junction (at 160.02 153.67) (diameter 0) (color 0 0 0 0))
  (wire (pts (xy 130.81 52.07) (xy 166.37 52.07)))
  (wire (pts (xy 209.55 142.24) (xy 209.55 139.7)))
  (wire (pts (xy 153.67 87.63) (xy 153.67 90.17)))
  (wire (pts (xy 224.79 44.45) (xy 208.28 44.45)))
  (wire (pts (xy 125.73 121.92) (xy 125.73 153.67)))
  (wire (pts (xy 118.11 26.67) (xy 184.15 26.67)))
  (wire (pts (xy 137.16 67.31) (xy 114.3 67.31)))
  (wire (pts (xy 246.38 133.35) (xy 262.89 133.35)))
  (wire (pts (xy 238.76 115.57) (xy 238.76 111.76)))
  (wire (pts (xy 220.98 139.7) (xy 238.76 139.7)))
  (wire (pts (xy 208.28 26.67) (xy 208.28 27.94)))
  (wire (pts (xy 205.74 52.07) (xy 208.28 52.07)))
  (wire (pts (xy 137.16 62.23) (xy 114.3 62.23)))
  (wire (pts (xy 262.89 22.86) (xy 262.89 115.57)))
  (wire (pts (xy 238.76 125.73) (xy 238.76 120.65)))
  (wire (pts (xy 114.3 67.31) (xy 114.3 90.17)))
  (wire (pts (xy 205.74 54.61) (xy 205.74 52.07)))
  (wire (pts (xy 125.73 153.67) (xy 146.05 153.67)))
  (wire (pts (xy 114.3 90.17) (xy 114.3 153.67)))
  (wire (pts (xy 144.78 62.23) (xy 151.13 62.23)))
  (wire (pts (xy 118.11 54.61) (xy 118.11 109.22)))
  (wire (pts (xy 128.27 49.53) (xy 128.27 57.15)))
  (wire (pts (xy 160.02 22.86) (xy 262.89 22.86)))
  (wire (pts (xy 181.61 87.63) (xy 208.28 87.63)))
  (wire (pts (xy 208.28 44.45) (xy 208.28 52.07)))
  (wire (pts (xy 205.74 54.61) (xy 191.77 54.61)))
  (wire (pts (xy 209.55 149.86) (xy 209.55 153.67)))
  (wire (pts (xy 156.21 67.31) (xy 166.37 67.31)))
  (wire (pts (xy 209.55 139.7) (xy 203.2 139.7)))
  (wire (pts (xy 160.02 57.15) (xy 160.02 22.86)))
  (wire (pts (xy 95.25 52.07) (xy 114.3 52.07)))
  (wire (pts (xy 166.37 57.15) (xy 160.02 57.15)))
  (wire (pts (xy 224.79 87.63) (xy 224.79 58.42)))
  (wire (pts (xy 146.05 152.4) (xy 146.05 153.67)))
  (wire (pts (xy 95.25 54.61) (xy 118.11 54.61)))
  (wire (pts (xy 209.55 139.7) (xy 220.98 139.7)))
  (wire (pts (xy 151.13 67.31) (xy 144.78 67.31)))
  (wire (pts (xy 238.76 153.67) (xy 238.76 148.59)))
  (wire (pts (xy 238.76 128.27) (xy 238.76 125.73)))
  (wire (pts (xy 238.76 139.7) (xy 238.76 138.43)))
  (wire (pts (xy 156.21 62.23) (xy 166.37 62.23)))
  (wire (pts (xy 128.27 49.53) (xy 166.37 49.53)))
  (wire (pts (xy 220.98 153.67) (xy 238.76 153.67)))
  (wire (pts (xy 262.89 133.35) (xy 262.89 125.73)))
  (wire (pts (xy 130.81 59.69) (xy 130.81 52.07)))
  (wire (pts (xy 203.2 139.7) (xy 203.2 59.69)))
  (wire (pts (xy 184.15 26.67) (xy 184.15 34.29)))
  (wire (pts (xy 153.67 77.47) (xy 153.67 74.93)))
  (wire (pts (xy 146.05 121.92) (xy 146.05 144.78)))
  (wire (pts (xy 220.98 147.32) (xy 220.98 153.67)))
  (wire (pts (xy 166.37 74.93) (xy 153.67 74.93)))
  (wire (pts (xy 208.28 33.02) (xy 208.28 44.45)))
  (wire (pts (xy 153.67 90.17) (xy 176.53 90.17)))
  (wire (pts (xy 209.55 153.67) (xy 220.98 153.67)))
  (wire (pts (xy 146.05 121.92) (xy 146.05 69.85)))
  (wire (pts (xy 238.76 146.05) (xy 238.76 139.7)))
  (wire (pts (xy 140.97 111.76) (xy 238.76 111.76)))
  (wire (pts (xy 118.11 54.61) (xy 118.11 26.67)))
  (wire (pts (xy 247.65 125.73) (xy 238.76 125.73)))
  (wire (pts (xy 114.3 52.07) (xy 114.3 62.23)))
  (wire (pts (xy 114.3 90.17) (xy 153.67 90.17)))
  (wire (pts (xy 146.05 121.92) (xy 140.97 121.92)))
  (wire (pts (xy 118.11 109.22) (xy 125.73 109.22)))
  (wire (pts (xy 160.02 153.67) (xy 209.55 153.67)))
  (wire (pts (xy 220.98 142.24) (xy 220.98 139.7)))
  (wire (pts (xy 208.28 87.63) (xy 208.28 57.15)))
  (wire (pts (xy 224.79 44.45) (xy 224.79 50.8)))
  (wire (pts (xy 95.25 57.15) (xy 128.27 57.15)))
  (wire (pts (xy 160.02 158.75) (xy 160.02 153.67)))
  (wire (pts (xy 184.15 26.67) (xy 208.28 26.67)))
  (wire (pts (xy 95.25 59.69) (xy 130.81 59.69)))
  (wire (pts (xy 252.73 125.73) (xy 262.89 125.73)))
  (wire (pts (xy 208.28 87.63) (xy 224.79 87.63)))
  (wire (pts (xy 262.89 125.73) (xy 262.89 120.65)))
  (wire (pts (xy 146.05 153.67) (xy 160.02 153.67)))
  (wire (pts (xy 146.05 69.85) (xy 166.37 69.85)))
  (wire (pts (xy 191.77 59.69) (xy 203.2 59.69)))
  (wire (pts (xy 114.3 153.67) (xy 125.73 153.67)))
  (wire (pts (xy 176.53 90.17) (xy 176.53 87.63)))
  (wire (pts (xy 114.3 62.23) (xy 114.3 67.31)))
  (text "Défaut" (at 130.81 62.23 0))
  (text "Charge" (at 130.81 67.31 0))
  (text "poussoir\n charge" (at 158.75 88.9 0))
  (symbol (lib_id "power:GND") (at 160.02 158.75 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "#PWR01" (id 0) (at 160.02 165.1 0))
    (property "Value" "" (id 1) (at 160.147 163.1442 0))
    (property "Footprint" "" (id 2) (at 160.02 158.75 0))
    (property "Datasheet" "" (id 3) (at 160.02 158.75 0))
    (pin "1")
  )
  (symbol (lib_id "MCU_Module:Arduino_UNO_R3") (at 179.07 59.69 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "A1" (id 0) (at 189.23 33.02 0))
    (property "Value" "" (id 1) (at 193.04 31.75 0))
    (property "Footprint" "" (id 2) (at 179.07 59.69 0))
    (property "Datasheet" "https://www.arduino.cc/en/Main/arduinoBoardUno" (id 3) (at 179.07 59.69 0))
    (pin "1")
    (pin "10")
    (pin "11")
    (pin "12")
    (pin "13")
    (pin "14")
    (pin "15")
    (pin "16")
    (pin "17")
    (pin "18")
    (pin "19")
    (pin "2")
    (pin "20")
    (pin "21")
    (pin "22")
    (pin "23")
    (pin "24")
    (pin "25")
    (pin "26")
    (pin "27")
    (pin "28")
    (pin "29")
    (pin "3")
    (pin "30")
    (pin "31")
    (pin "32")
    (pin "4")
    (pin "5")
    (pin "6")
    (pin "7")
    (pin "8")
    (pin "9")
  )
  (symbol (lib_id "kicad_chargeur_piles_mosfet-rescue:Display_TM1637-display_tm1637-kicad_chargeur_piles-rescue") (at 67.31 49.53 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "U1" (id 0) (at 68.58 34.29 0))
    (property "Value" "" (id 1) (at 68.7578 34.8996 0))
    (property "Footprint" "" (id 2) (at 67.31 64.77 0))
    (property "Datasheet" "http://www.kingbright.com/attachments/file/psearch/000/00/00/CC56-12CGKWA(Ver.8A).pdf" (id 3) (at 56.388 48.768 0))
    (pin "1")
    (pin "2")
    (pin "3")
    (pin "4")
  )
  (symbol (lib_id "Relay:SANYOU_SRD_Form_C") (at 133.35 116.84 90) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "K1" (id 0) (at 133.35 104.14 90))
    (property "Value" "" (id 1) (at 135.89 104.14 90))
    (property "Footprint" "" (id 2) (at 134.62 105.41 0))
    (property "Datasheet" "http://www.sanyourelay.ca/public/products/pdf/SRD.pdf" (id 3) (at 133.35 116.84 0))
    (pin "1")
    (pin "2")
    (pin "3")
    (pin "4")
    (pin "5")
  )
  (symbol (lib_id "Diode:1N4004") (at 146.05 148.59 270) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "D1" (id 0) (at 148.082 147.4216 90))
    (property "Value" "" (id 1) (at 148.082 149.733 90))
    (property "Footprint" "" (id 2) (at 141.605 148.59 0))
    (property "Datasheet" "http://www.vishay.com/docs/88503/1n4001.pdf" (id 3) (at 146.05 148.59 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "Device:R_Small") (at 153.67 62.23 270) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "R3" (id 0) (at 153.67 59.5884 90))
    (property "Value" "" (id 1) (at 153.67 59.563 90))
    (property "Footprint" "" (id 2) (at 153.67 62.23 0))
    (property "Datasheet" "~" (id 3) (at 153.67 62.23 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "Device:R_Small") (at 153.67 67.31 270) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "R2" (id 0) (at 153.67 64.6684 90))
    (property "Value" "" (id 1) (at 153.67 64.643 90))
    (property "Footprint" "" (id 2) (at 153.67 67.31 0))
    (property "Datasheet" "~" (id 3) (at 153.67 67.31 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "Device:LED") (at 140.97 62.23 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "D3" (id 0) (at 144.78 60.96 0))
    (property "Value" "" (id 1) (at 140.7922 59.0296 0))
    (property "Footprint" "" (id 2) (at 140.97 62.23 0))
    (property "Datasheet" "~" (id 3) (at 140.97 62.23 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "Device:LED") (at 140.97 67.31 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "D2" (id 0) (at 144.78 66.04 0))
    (property "Value" "" (id 1) (at 140.7922 64.1096 0))
    (property "Footprint" "" (id 2) (at 140.97 67.31 0))
    (property "Datasheet" "~" (id 3) (at 140.97 67.31 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "Connector_Generic:Conn_01x02") (at 243.84 146.05 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "J1" (id 0) (at 242.57 142.24 0))
    (property "Value" "" (id 1) (at 234.95 152.4 0))
    (property "Footprint" "" (id 2) (at 243.84 146.05 0))
    (property "Datasheet" "~" (id 3) (at 243.84 146.05 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "Device:R_Small") (at 238.76 118.11 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "R4" (id 0) (at 240.2586 118.11 0))
    (property "Value" "" (id 1) (at 240.2586 119.253 0))
    (property "Footprint" "" (id 2) (at 238.76 118.11 0))
    (property "Datasheet" "~" (id 3) (at 238.76 118.11 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "Device:Q_PMOS_GDS") (at 241.3 133.35 180) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "Q1" (id 0) (at 236.093 132.1816 0))
    (property "Value" "" (id 1) (at 236.093 134.493 0))
    (property "Footprint" "" (id 2) (at 236.22 135.89 0))
    (property "Datasheet" "~" (id 3) (at 241.3 133.35 0))
    (pin "1")
    (pin "2")
    (pin "3")
  )
  (symbol (lib_id "Device:R_Small") (at 262.89 118.11 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "R6" (id 0) (at 264.3886 118.11 0))
    (property "Value" "" (id 1) (at 264.3886 119.253 0))
    (property "Footprint" "" (id 2) (at 262.89 118.11 0))
    (property "Datasheet" "~" (id 3) (at 262.89 118.11 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "Device:R_Small") (at 220.98 144.78 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "R1" (id 0) (at 222.4786 144.78 0))
    (property "Value" "" (id 1) (at 222.4786 145.923 0))
    (property "Footprint" "" (id 2) (at 220.98 144.78 0))
    (property "Datasheet" "~" (id 3) (at 220.98 144.78 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "Device:C") (at 209.55 146.05 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "C1" (id 0) (at 212.471 146.05 0))
    (property "Value" "" (id 1) (at 212.471 147.193 0))
    (property "Footprint" "" (id 2) (at 210.5152 149.86 0))
    (property "Datasheet" "~" (id 3) (at 209.55 146.05 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "Device:R_Small") (at 250.19 125.73 270) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "R5" (id 0) (at 248.92 121.92 90))
    (property "Value" "" (id 1) (at 249.047 127.2286 0))
    (property "Footprint" "" (id 2) (at 250.19 125.73 0))
    (property "Datasheet" "~" (id 3) (at 250.19 125.73 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "Reference_Voltage:TL431LP") (at 208.28 54.61 90) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "U2" (id 0) (at 210.058 53.4416 90))
    (property "Value" "" (id 1) (at 210.058 55.753 90))
    (property "Footprint" "" (id 2) (at 212.09 54.61 0))
    (property "Datasheet" "http://www.ti.com/lit/ds/symlink/tl431.pdf" (id 3) (at 208.28 54.61 0))
    (pin "1")
    (pin "2")
    (pin "3")
  )
  (symbol (lib_id "Device:R_Small") (at 208.28 30.48 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "R7" (id 0) (at 209.7786 30.48 0))
    (property "Value" "" (id 1) (at 209.7786 31.623 0))
    (property "Footprint" "" (id 2) (at 208.28 30.48 0))
    (property "Datasheet" "~" (id 3) (at 208.28 30.48 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "Connector:TestPoint_2Pole") (at 153.67 82.55 270) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "TP1" (id 0) (at 155.1432 82.55 90))
    (property "Value" "" (id 1) (at 155.1432 83.693 90))
    (property "Footprint" "" (id 2) (at 153.67 82.55 0))
    (property "Datasheet" "~" (id 3) (at 153.67 82.55 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "Device:C_Polarized") (at 224.79 54.61 0) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "C2" (id 0) (at 228.6 52.4509 0))
    (property "Value" "" (id 1) (at 228.6 54.9909 0))
    (property "Footprint" "" (id 2) (at 225.7552 58.42 0))
    (property "Datasheet" "~" (id 3) (at 224.79 54.61 0))
    (pin "1")
    (pin "2")
  )
  (sheet_instances
    (path (page "1"))
  )
  (symbol_instances
    (path
      (reference "#PWR01") (unit 1) (value "GND") (footprint "")
    )
    (path
      (reference "A1") (unit 1) (value "Arduino_UNO_R3") (footprint "kicad_chargeur_piles:Arduino_UNO_R3")
    )
    (path
      (reference "C1") (unit 1) (value "C") (footprint "Capacitor_THT:C_Rect_L7.0mm_W2.0mm_P5.00mm")
    )
    (path
      (reference "C2") (unit 1) (value "C_Polarized") (footprint "Capacitor_THT:CP_Radial_Tantal_D6.0mm_P2.50mm")
    )
    (path
      (reference "D1") (unit 1) (value "1N4001") (footprint "Diode_THT:D_DO-41_SOD81_P10.16mm_Horizontal")
    )
    (path
      (reference "D2") (unit 1) (value "LED verte") (footprint "LED_THT:LED_D3.0mm")
    )
    (path
      (reference "D3") (unit 1) (value "LED Rouge") (footprint "LED_THT:LED_D3.0mm")
    )
    (path
      (reference "J1") (unit 1) (value "Conn_01x02") (footprint "TerminalBlock_Phoenix:TerminalBlock_Phoenix_MKDS-1,5-2_1x02_P5.00mm_Horizontal")
    )
    (path
      (reference "K1") (unit 1) (value "SRD-5VDC") (footprint "Relay_THT:Relay_SPDT_SANYOU_SRD_Series_Form_C")
    )
    (path
      (reference "Q1") (unit 1) (value "Q_PMOS_GDS") (footprint "Package_TO_SOT_THT:TO-220-3_Horizontal_TabDown")
    )
    (path
      (reference "R1") (unit 1) (value "R_Small") (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal")
    )
    (path
      (reference "R2") (unit 1) (value "R_Small") (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal")
    )
    (path
      (reference "R3") (unit 1) (value "R_Small") (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal")
    )
    (path
      (reference "R4") (unit 1) (value "R_Small") (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal")
    )
    (path
      (reference "R5") (unit 1) (value "R_Small") (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal")
    )
    (path
      (reference "R6") (unit 1) (value "R_Small") (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal")
    )
    (path
      (reference "R7") (unit 1) (value "R_Small") (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal")
    )
    (path
      (reference "TP1") (unit 1) (value "TestPoint_2Pole") (footprint "Connector_PinHeader_1.00mm:PinHeader_1x02_P1.00mm_Vertical")
    )
    (path
      (reference "U1") (unit 1) (value "Display_TM1637") (footprint "kicad_chargeur_piles:Display_TM1637")
    )
    (path
      (reference "U2") (unit 1) (value "TL431LP") (footprint "Package_TO_SOT_THT:TO-92_Inline")
    )
  )
)
